\hypertarget{classmod__oasis__getput__interface}{\section{mod\+\_\+oasis\+\_\+getput\+\_\+interface Module Reference}
\label{classmod__oasis__getput__interface}\index{mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}}
}


O\+A\+S\+I\+S send/receive (put/get) user interfaces.  


\subsection*{Data Types}
\begin{DoxyCompactItemize}
\item 
interface \hyperlink{interfacemod__oasis__getput__interface_1_1oasis__get}{oasis\+\_\+get}
\begin{DoxyCompactList}\small\item\em Generic overloaded interface for data get (receive) \end{DoxyCompactList}\item 
interface \hyperlink{interfacemod__oasis__getput__interface_1_1oasis__put}{oasis\+\_\+put}
\begin{DoxyCompactList}\small\item\em Generic overloaded interface for data put (send) \end{DoxyCompactList}\end{DoxyCompactItemize}
\subsection*{Private Member Functions}
\begin{DoxyCompactItemize}
\item 
subroutine \hyperlink{classmod__oasis__getput__interface_a3ecaceac872ddf003a810f26b4c03f28}{oasis\+\_\+put\+\_\+r14} (id\+\_\+port\+\_\+id, kstep, fld1, kinfo, fld2, fld3, fld4, fld5)
\begin{DoxyCompactList}\small\item\em Send 4 byte real 1\+D data. \end{DoxyCompactList}\item 
subroutine \hyperlink{classmod__oasis__getput__interface_a021f5e4f2baa2e729816e97c6cf8df4d}{oasis\+\_\+put\+\_\+r18} (id\+\_\+port\+\_\+id, kstep, fld1, kinfo, fld2, fld3, fld4, fld5)
\begin{DoxyCompactList}\small\item\em Send 8 byte real 1\+D data. \end{DoxyCompactList}\item 
subroutine \hyperlink{classmod__oasis__getput__interface_a4536f2b61cf8190bf83f7dbf3dae9eb5}{oasis\+\_\+put\+\_\+r24} (id\+\_\+port\+\_\+id, kstep, fld1, kinfo, fld2, fld3, fld4, fld5)
\begin{DoxyCompactList}\small\item\em Send 4 byte real 2\+D data. \end{DoxyCompactList}\item 
subroutine \hyperlink{classmod__oasis__getput__interface_a3fa517cd2498afe1e0e38b58d186ee53}{oasis\+\_\+put\+\_\+r28} (id\+\_\+port\+\_\+id, kstep, fld1, kinfo, fld2, fld3, fld4, fld5)
\begin{DoxyCompactList}\small\item\em Send 8 byte real 2\+D data. \end{DoxyCompactList}\item 
subroutine \hyperlink{classmod__oasis__getput__interface_a2c56f0b77e74cceed2553583f6ccb2a2}{oasis\+\_\+get\+\_\+r14} (id\+\_\+port\+\_\+id, kstep, rd\+\_\+field, kinfo)
\begin{DoxyCompactList}\small\item\em Receive 4 byte real 1\+D data. \end{DoxyCompactList}\item 
subroutine \hyperlink{classmod__oasis__getput__interface_a11a6b191557bac5677f77c8af755958b}{oasis\+\_\+get\+\_\+r18} (id\+\_\+port\+\_\+id, kstep, rd\+\_\+field, kinfo)
\begin{DoxyCompactList}\small\item\em Receive 8 byte real 1\+D data. \end{DoxyCompactList}\item 
subroutine \hyperlink{classmod__oasis__getput__interface_adb63a11f1dc98b61159747ce37af7a86}{oasis\+\_\+get\+\_\+r24} (id\+\_\+port\+\_\+id, kstep, rd\+\_\+field, kinfo)
\begin{DoxyCompactList}\small\item\em Receive 4 byte real 2\+D data. \end{DoxyCompactList}\item 
subroutine \hyperlink{classmod__oasis__getput__interface_a7178554f023eb62092fb03e2edf55eb6}{oasis\+\_\+get\+\_\+r28} (id\+\_\+port\+\_\+id, kstep, rd\+\_\+field, kinfo)
\begin{DoxyCompactList}\small\item\em Receive 8 byte real 2\+D data. \end{DoxyCompactList}\end{DoxyCompactItemize}
\subsection*{Private Attributes}
\begin{DoxyCompactItemize}
\item 
integer(kind=ip\+\_\+i4\+\_\+p), \\*
dimension(mpi\+\_\+status\+\_\+size) \hyperlink{classmod__oasis__getput__interface_a2ceaaa5740216799f651b8dacb42b239}{istatus}
\end{DoxyCompactItemize}


\subsection{Detailed Description}
O\+A\+S\+I\+S send/receive (put/get) user interfaces. 

Definition at line 4 of file mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90.



\subsection{Member Function/\+Subroutine Documentation}
\hypertarget{classmod__oasis__getput__interface_a2c56f0b77e74cceed2553583f6ccb2a2}{\index{mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}!oasis\+\_\+get\+\_\+r14@{oasis\+\_\+get\+\_\+r14}}
\index{oasis\+\_\+get\+\_\+r14@{oasis\+\_\+get\+\_\+r14}!mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}}
\subsubsection[{oasis\+\_\+get\+\_\+r14}]{\setlength{\rightskip}{0pt plus 5cm}subroutine mod\+\_\+oasis\+\_\+getput\+\_\+interface\+::oasis\+\_\+get\+\_\+r14 (
\begin{DoxyParamCaption}
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{id\+\_\+port\+\_\+id, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{kstep, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:), intent(inout)}]{rd\+\_\+field, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(out), optional}]{kinfo}
\end{DoxyParamCaption}
)\hspace{0.3cm}{\ttfamily [private]}}}\label{classmod__oasis__getput__interface_a2c56f0b77e74cceed2553583f6ccb2a2}


Receive 4 byte real 1\+D data. 


\begin{DoxyParams}[1]{Parameters}
\mbox{\tt in}  & {\em id\+\_\+port\+\_\+id} & variable id\\
\hline
\mbox{\tt in}  & {\em kstep} & model time in seconds\\
\hline
\mbox{\tt in,out}  & {\em rd\+\_\+field} & field data\\
\hline
\mbox{\tt out}  & {\em kinfo} & return code \\
\hline
\end{DoxyParams}


Definition at line 643 of file mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90.

\hypertarget{classmod__oasis__getput__interface_a11a6b191557bac5677f77c8af755958b}{\index{mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}!oasis\+\_\+get\+\_\+r18@{oasis\+\_\+get\+\_\+r18}}
\index{oasis\+\_\+get\+\_\+r18@{oasis\+\_\+get\+\_\+r18}!mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}}
\subsubsection[{oasis\+\_\+get\+\_\+r18}]{\setlength{\rightskip}{0pt plus 5cm}subroutine mod\+\_\+oasis\+\_\+getput\+\_\+interface\+::oasis\+\_\+get\+\_\+r18 (
\begin{DoxyParamCaption}
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{id\+\_\+port\+\_\+id, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{kstep, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:), intent(inout)}]{rd\+\_\+field, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(out), optional}]{kinfo}
\end{DoxyParamCaption}
)\hspace{0.3cm}{\ttfamily [private]}}}\label{classmod__oasis__getput__interface_a11a6b191557bac5677f77c8af755958b}


Receive 8 byte real 1\+D data. 


\begin{DoxyParams}[1]{Parameters}
\mbox{\tt in}  & {\em id\+\_\+port\+\_\+id} & variable id\\
\hline
\mbox{\tt in}  & {\em kstep} & model time in seconds\\
\hline
\mbox{\tt in,out}  & {\em rd\+\_\+field} & field data\\
\hline
\mbox{\tt out}  & {\em kinfo} & return code \\
\hline
\end{DoxyParams}


Definition at line 716 of file mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90.

\hypertarget{classmod__oasis__getput__interface_adb63a11f1dc98b61159747ce37af7a86}{\index{mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}!oasis\+\_\+get\+\_\+r24@{oasis\+\_\+get\+\_\+r24}}
\index{oasis\+\_\+get\+\_\+r24@{oasis\+\_\+get\+\_\+r24}!mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}}
\subsubsection[{oasis\+\_\+get\+\_\+r24}]{\setlength{\rightskip}{0pt plus 5cm}subroutine mod\+\_\+oasis\+\_\+getput\+\_\+interface\+::oasis\+\_\+get\+\_\+r24 (
\begin{DoxyParamCaption}
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{id\+\_\+port\+\_\+id, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{kstep, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:,\+:), intent(inout)}]{rd\+\_\+field, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(out), optional}]{kinfo}
\end{DoxyParamCaption}
)\hspace{0.3cm}{\ttfamily [private]}}}\label{classmod__oasis__getput__interface_adb63a11f1dc98b61159747ce37af7a86}


Receive 4 byte real 2\+D data. 


\begin{DoxyParams}[1]{Parameters}
\mbox{\tt in}  & {\em id\+\_\+port\+\_\+id} & variable id\\
\hline
\mbox{\tt in}  & {\em kstep} & model time in seconds\\
\hline
\mbox{\tt in,out}  & {\em rd\+\_\+field} & field data\\
\hline
\mbox{\tt out}  & {\em kinfo} & return code \\
\hline
\end{DoxyParams}


Definition at line 779 of file mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90.

\hypertarget{classmod__oasis__getput__interface_a7178554f023eb62092fb03e2edf55eb6}{\index{mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}!oasis\+\_\+get\+\_\+r28@{oasis\+\_\+get\+\_\+r28}}
\index{oasis\+\_\+get\+\_\+r28@{oasis\+\_\+get\+\_\+r28}!mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}}
\subsubsection[{oasis\+\_\+get\+\_\+r28}]{\setlength{\rightskip}{0pt plus 5cm}subroutine mod\+\_\+oasis\+\_\+getput\+\_\+interface\+::oasis\+\_\+get\+\_\+r28 (
\begin{DoxyParamCaption}
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{id\+\_\+port\+\_\+id, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{kstep, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:,\+:), intent(inout)}]{rd\+\_\+field, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(out), optional}]{kinfo}
\end{DoxyParamCaption}
)\hspace{0.3cm}{\ttfamily [private]}}}\label{classmod__oasis__getput__interface_a7178554f023eb62092fb03e2edf55eb6}


Receive 8 byte real 2\+D data. 


\begin{DoxyParams}[1]{Parameters}
\mbox{\tt in}  & {\em id\+\_\+port\+\_\+id} & variable id\\
\hline
\mbox{\tt in}  & {\em kstep} & model time in seconds\\
\hline
\mbox{\tt in,out}  & {\em rd\+\_\+field} & field data\\
\hline
\mbox{\tt out}  & {\em kinfo} & return code \\
\hline
\end{DoxyParams}


Definition at line 854 of file mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90.

\hypertarget{classmod__oasis__getput__interface_a3ecaceac872ddf003a810f26b4c03f28}{\index{mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}!oasis\+\_\+put\+\_\+r14@{oasis\+\_\+put\+\_\+r14}}
\index{oasis\+\_\+put\+\_\+r14@{oasis\+\_\+put\+\_\+r14}!mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}}
\subsubsection[{oasis\+\_\+put\+\_\+r14}]{\setlength{\rightskip}{0pt plus 5cm}subroutine mod\+\_\+oasis\+\_\+getput\+\_\+interface\+::oasis\+\_\+put\+\_\+r14 (
\begin{DoxyParamCaption}
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{id\+\_\+port\+\_\+id, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{kstep, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:)}]{fld1, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(out), optional}]{kinfo, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:), optional}]{fld2, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:), optional}]{fld3, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:), optional}]{fld4, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:), optional}]{fld5}
\end{DoxyParamCaption}
)\hspace{0.3cm}{\ttfamily [private]}}}\label{classmod__oasis__getput__interface_a3ecaceac872ddf003a810f26b4c03f28}


Send 4 byte real 1\+D data. 


\begin{DoxyParams}[1]{Parameters}
\mbox{\tt in}  & {\em id\+\_\+port\+\_\+id} & variable id\\
\hline
\mbox{\tt in}  & {\em kstep} & model time in seconds\\
\hline
 & {\em fld1} & field data\\
\hline
\mbox{\tt out}  & {\em kinfo} & return code\\
\hline
 & {\em fld2} & higher order field data\\
\hline
 & {\em fld3} & higher order field data\\
\hline
 & {\em fld4} & higher order field data\\
\hline
 & {\em fld5} & higher order field data \\
\hline
\end{DoxyParams}


Definition at line 52 of file mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90.

\hypertarget{classmod__oasis__getput__interface_a021f5e4f2baa2e729816e97c6cf8df4d}{\index{mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}!oasis\+\_\+put\+\_\+r18@{oasis\+\_\+put\+\_\+r18}}
\index{oasis\+\_\+put\+\_\+r18@{oasis\+\_\+put\+\_\+r18}!mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}}
\subsubsection[{oasis\+\_\+put\+\_\+r18}]{\setlength{\rightskip}{0pt plus 5cm}subroutine mod\+\_\+oasis\+\_\+getput\+\_\+interface\+::oasis\+\_\+put\+\_\+r18 (
\begin{DoxyParamCaption}
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{id\+\_\+port\+\_\+id, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{kstep, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:)}]{fld1, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(out), optional}]{kinfo, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:), optional}]{fld2, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:), optional}]{fld3, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:), optional}]{fld4, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:), optional}]{fld5}
\end{DoxyParamCaption}
)\hspace{0.3cm}{\ttfamily [private]}}}\label{classmod__oasis__getput__interface_a021f5e4f2baa2e729816e97c6cf8df4d}


Send 8 byte real 1\+D data. 


\begin{DoxyParams}[1]{Parameters}
\mbox{\tt in}  & {\em id\+\_\+port\+\_\+id} & variable id\\
\hline
\mbox{\tt in}  & {\em kstep} & model time in seconds\\
\hline
 & {\em fld1} & field data\\
\hline
\mbox{\tt out}  & {\em kinfo} & return code\\
\hline
 & {\em fld2} & higher order field data\\
\hline
 & {\em fld3} & higher order field data\\
\hline
 & {\em fld4} & higher order field data\\
\hline
 & {\em fld5} & higher order field data \\
\hline
\end{DoxyParams}


Definition at line 197 of file mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90.

\hypertarget{classmod__oasis__getput__interface_a4536f2b61cf8190bf83f7dbf3dae9eb5}{\index{mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}!oasis\+\_\+put\+\_\+r24@{oasis\+\_\+put\+\_\+r24}}
\index{oasis\+\_\+put\+\_\+r24@{oasis\+\_\+put\+\_\+r24}!mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}}
\subsubsection[{oasis\+\_\+put\+\_\+r24}]{\setlength{\rightskip}{0pt plus 5cm}subroutine mod\+\_\+oasis\+\_\+getput\+\_\+interface\+::oasis\+\_\+put\+\_\+r24 (
\begin{DoxyParamCaption}
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{id\+\_\+port\+\_\+id, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{kstep, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:,\+:)}]{fld1, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(out), optional}]{kinfo, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:,\+:), optional}]{fld2, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:,\+:), optional}]{fld3, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:,\+:), optional}]{fld4, }
\item[{real(kind=ip\+\_\+single\+\_\+p), dimension(\+:,\+:), optional}]{fld5}
\end{DoxyParamCaption}
)\hspace{0.3cm}{\ttfamily [private]}}}\label{classmod__oasis__getput__interface_a4536f2b61cf8190bf83f7dbf3dae9eb5}


Send 4 byte real 2\+D data. 


\begin{DoxyParams}[1]{Parameters}
\mbox{\tt in}  & {\em id\+\_\+port\+\_\+id} & variable id\\
\hline
\mbox{\tt in}  & {\em kstep} & model time in seconds\\
\hline
 & {\em fld1} & field data\\
\hline
\mbox{\tt out}  & {\em kinfo} & return code\\
\hline
 & {\em fld2} & higher order field data\\
\hline
 & {\em fld3} & higher order field data\\
\hline
 & {\em fld4} & higher order field data\\
\hline
 & {\em fld5} & higher order field data \\
\hline
\end{DoxyParams}


Definition at line 341 of file mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90.

\hypertarget{classmod__oasis__getput__interface_a3fa517cd2498afe1e0e38b58d186ee53}{\index{mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}!oasis\+\_\+put\+\_\+r28@{oasis\+\_\+put\+\_\+r28}}
\index{oasis\+\_\+put\+\_\+r28@{oasis\+\_\+put\+\_\+r28}!mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}}
\subsubsection[{oasis\+\_\+put\+\_\+r28}]{\setlength{\rightskip}{0pt plus 5cm}subroutine mod\+\_\+oasis\+\_\+getput\+\_\+interface\+::oasis\+\_\+put\+\_\+r28 (
\begin{DoxyParamCaption}
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{id\+\_\+port\+\_\+id, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(in)}]{kstep, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:,\+:)}]{fld1, }
\item[{integer(kind=ip\+\_\+i4\+\_\+p), intent(out), optional}]{kinfo, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:,\+:), optional}]{fld2, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:,\+:), optional}]{fld3, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:,\+:), optional}]{fld4, }
\item[{real(kind=ip\+\_\+double\+\_\+p), dimension(\+:,\+:), optional}]{fld5}
\end{DoxyParamCaption}
)\hspace{0.3cm}{\ttfamily [private]}}}\label{classmod__oasis__getput__interface_a3fa517cd2498afe1e0e38b58d186ee53}


Send 8 byte real 2\+D data. 


\begin{DoxyParams}[1]{Parameters}
\mbox{\tt in}  & {\em id\+\_\+port\+\_\+id} & variable id\\
\hline
\mbox{\tt in}  & {\em kstep} & model time in seconds\\
\hline
 & {\em fld1} & field data\\
\hline
\mbox{\tt out}  & {\em kinfo} & return code\\
\hline
 & {\em fld2} & higher order field data\\
\hline
 & {\em fld3} & higher order field data\\
\hline
 & {\em fld4} & higher order field data\\
\hline
 & {\em fld5} & higher order field data \\
\hline
\end{DoxyParams}


Definition at line 492 of file mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90.



\subsection{Member Data Documentation}
\hypertarget{classmod__oasis__getput__interface_a2ceaaa5740216799f651b8dacb42b239}{\index{mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}!istatus@{istatus}}
\index{istatus@{istatus}!mod\+\_\+oasis\+\_\+getput\+\_\+interface@{mod\+\_\+oasis\+\_\+getput\+\_\+interface}}
\subsubsection[{istatus}]{\setlength{\rightskip}{0pt plus 5cm}integer(kind=ip\+\_\+i4\+\_\+p), dimension(mpi\+\_\+status\+\_\+size) mod\+\_\+oasis\+\_\+getput\+\_\+interface\+::istatus\hspace{0.3cm}{\ttfamily [private]}}}\label{classmod__oasis__getput__interface_a2ceaaa5740216799f651b8dacb42b239}


Definition at line 23 of file mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90.



The documentation for this module was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
/\+Users/tcraig/\+Desktop/oasis/oasis3-\/mct.\+trunk/lib/psmile/src/\hyperlink{mod__oasis__getput__interface_8_f90}{mod\+\_\+oasis\+\_\+getput\+\_\+interface.\+F90}\end{DoxyCompactItemize}
